**Recording Impedance from PZ5 128 Neuro Digitizer**

Kevin O’Neill

2014/10/30

**Summary:**

This document will demonstrate how to record impedance values from the PZ5 128 Neuro Digitizer

**Procedure:**

1. Turn on all equipment (RZ2, RZ5D, PC, PZ5)
2. Open ‘ImpedanceTest’ from the workbench
3. Change Block name
4. Preview the .rcx
5. Switch PZ5 to impedance testing mode
6. Select frequency on the PZ5
7. Record the data from the Workbench